Microsoft Windows [Version 6.1.7601]
Copyright (c) 2009 Microsoft Corporation.  All rights reserved.

C:\BACnet\Bin>bacrpm 200121 8 200121 120
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    vendor-identifier: 648
}

C:\BACnet\Bin>bacrpm 200121 8 200121 70
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    model-name: "2080sc-BACNET"
}

C:\BACnet\Bin>bacrpm 200121 8 200121 44
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    firmware-revision: "0.6.0"
}

C:\BACnet\Bin>bacrpm 200121 8 200121 12
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    application-software-version: "1.11"
}

C:\BACnet\Bin>bacrpm 200121 8 200121 98
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    protocol-version: 1
}

C:\BACnet\Bin>bacrpm 200121 8 200121 139
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    protocol-revision: 10
}

C:\BACnet\Bin>bacrpm 200121 8 200121 97
host: sciwin7-AF2 at 192.168.2.98
IP Address: 192.168.2.98
IP Broadcast Address: 255.255.255.255
UDP Port: 0xBAC0 [47808]
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device #200121
{
    protocol-services-supported: {false,false,false,false,false,false,false,fals
e,false,false,false,false,true,false,true,true,true,true,false,false,true,false,
false,false,false,false,false,false,false,false,false,false,true,true,true,false
,true,false,false,false}
}

C:\BACnet\Bin>