host: WIN10-AF1 at 192.168.2.249
BVLC: Sent Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Received Original-Broadcast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
PICS 0

BACnet Protocol Implementation Conformance Statement



--

--

-- BACnet/IP Interface for BACnet-stack Devices

-- http://sourceforge.net/projects/bacnet/ 

-- 

-- 



Vendor Name: "Spectrum Controls Inc"

Product Name: "2080sc-BACNET"

Product Model Number: "2080sc-BACNET"

Product Description: "Spectrum Controls 2080 BACnet Module"



BIBBs Supported:

{

 DS-RP-B

 DS-RPM-B

 DS-WP-B

 DM-DDB-B

 DM-DOB-B

 DM-DCC-B

 DM-RD-B

}



BACnet Standard Application Services Supported:

{

 ReadProperty                   Initiate Execute

 ReadPropertyMultiple           Execute

 WriteProperty                  Execute

 DeviceCommunicationControl     Execute

 Who-Has                        Execute

 I-Have                         Initiate

 Who-Is                         Initiate Execute

 I-Am                           Initiate

 ReinitializeDevice             Execute

}



Standard Object-Types Supported:

{

 Analog Input

 Analog Output

 Binary Input

 Binary Output

 Device

}



Data Link Layer Option:

{

 BACnet/IP, 'DIX' Ethernet

}



Character Sets Supported:

{

 ANSI X3.4

}



Special Functionality:

{

 Maximum APDU size in octets: 1476

}



List of Objects in Test Device:

{

  {

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
(Device, 96) Writable

    object-name: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
"Spectrum_BACNET" Writable

    object-type: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
Device

    system-status: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
operational

    vendor-name: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
"Spectrum Controls Inc"

    vendor-identifier: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
648

    model-name: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
"2080sc-BACNET"

    firmware-revision: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
"0.6.0"

    application-software-version: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
"2.0."

    protocol-version: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
1

    protocol-revision: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
10

    protocol-services-supported: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
( 

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        T,F,T,T,   --  Read-Property,, Read-Property-Multiple, Write-Property,

        T,T,F,F,   --  Write-Property-Multiple, Device-Communication-Control,,,

        T,F,F,F,   --  Reinitialize-Device,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        T,T,T,F,   --  Time-Synchronization, Who-Has, Who-Is,,

        T,F,F,F    --  UTC-Time-Synchronization,,,,

        ) 

    protocol-object-types-supported: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
( 

        T,T,F,T,   --  Analog Input, Analog Output,, Binary Input,

        T,F,F,F,   --  Binary Output,,,,

        T,F,F,F,   --  Device,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F,F,   -- ,,,,

        F,F,F    -- ,,,

        ) 

    object-list: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
{ 

        (Device, 96), (Analog Input, 0), (Analog Input, 1), (Analog Input, 2), 

        (Analog Input, 3), (Analog Input, 4), (Analog Input, 5), (Analog Input, 6), 

        (Analog Input, 7), (Analog Input, 8), (Analog Input, 9), (Analog Input, 10), 

        (Analog Input, 11), (Analog Input, 12), (Analog Input, 13), (Analog Input, 14), 

        (Analog Input, 15), (Analog Input, 16), (Analog Input, 17), (Analog Input, 18), 

        (Analog Input, 19), (Analog Input, 20), (Analog Input, 21), (Analog Input, 22), 

        (Analog Input, 23), (Analog Input, 24), (Analog Input, 25), (Analog Input, 26), 

        (Analog Input, 27), (Analog Input, 28), (Analog Input, 29), (Analog Input, 30), 

        (Analog Input, 31), (Analog Input, 32), (Analog Input, 33), (Analog Input, 34), 

        (Analog Input, 35), (Analog Input, 36), (Analog Input, 37), (Analog Input, 38), 

        (Analog Input, 39), (Analog Input, 40), (Analog Input, 41), (Analog Input, 42), 

        (Analog Input, 43), (Analog Input, 44), (Analog Input, 45), (Analog Input, 46), 

        (Analog Input, 47), (Analog Input, 48), (Analog Input, 49), (Analog Input, 50), 

        (Analog Input, 51), (Analog Input, 52), (Analog Input, 53), (Analog Input, 54), 

        (Analog Input, 55), (Analog Input, 56), (Analog Input, 57), (Analog Input, 58), 

        (Analog Input, 59), (Analog Input, 60), (Analog Input, 61), (Analog Input, 62), 

        (Analog Input, 63), (Analog Output, 0), (Analog Output, 1), (Analog Output, 2), 

        (Analog Output, 3), (Analog Output, 4), (Analog Output, 5), (Analog Output, 6), 

        (Analog Output, 7), (Analog Output, 8), (Analog Output, 9), (Analog Output, 10), 

        (Analog Output, 11), (Analog Output, 12), (Analog Output, 13), (Analog Output, 14), 

        (Analog Output, 15), (Analog Output, 16), (Analog Output, 17), (Analog Output, 18), 

        (Analog Output, 19), (Analog Output, 20), (Analog Output, 21), (Analog Output, 22), 

        (Analog Output, 23), (Analog Output, 24), (Analog Output, 25), (Analog Output, 26), 

        (Analog Output, 27), (Analog Output, 28), (Analog Output, 29), (Analog Output, 30), 

        (Analog Output, 31), (Analog Output, 32), (Analog Output, 33), (Analog Output, 34), 

        (Analog Output, 35), (Analog Output, 36), (Analog Output, 37), (Analog Output, 38), 

        (Analog Output, 39), (Analog Output, 40), (Analog Output, 41), (Analog Output, 42), 

        (Analog Output, 43), (Analog Output, 44), (Analog Output, 45), (Analog Output, 46), 

        (Analog Output, 47), (Analog Output, 48), (Analog Output, 49), (Analog Output, 50), 

        (Analog Output, 51), (Analog Output, 52), (Analog Output, 53), (Analog Output, 54), 

        (Analog Output, 55), (Analog Output, 56), (Analog Output, 57), (Analog Output, 58), 

        (Analog Output, 59), (Analog Output, 60), (Analog Output, 61), (Analog Output, 62), 

        (Analog Output, 63), (Binary Input, 0), (Binary Input, 1), (Binary Input, 2), 

        (Binary Input, 3), (Binary Input, 4), (Binary Input, 5), (Binary Input, 6), 

        (Binary Input, 7), (Binary Input, 8), (Binary Input, 9), (Binary Input, 10), 

        (Binary Input, 11), (Binary Input, 12), (Binary Input, 13), (Binary Input, 14), 

        (Binary Input, 15), (Binary Input, 16), (Binary Input, 17), (Binary Input, 18), 

        (Binary Input, 19), (Binary Input, 20), (Binary Input, 21), (Binary Input, 22), 

        (Binary Input, 23), (Binary Input, 24), (Binary Input, 25), (Binary Input, 26), 

        (Binary Input, 27), (Binary Input, 28), (Binary Input, 29), (Binary Input, 30), 

        (Binary Input, 31), (Binary Input, 32), (Binary Input, 33), (Binary Input, 34), 

        (Binary Input, 35), (Binary Input, 36), (Binary Input, 37), (Binary Input, 38), 

        (Binary Input, 39), (Binary Input, 40), (Binary Input, 41), (Binary Input, 42), 

        (Binary Input, 43), (Binary Input, 44), (Binary Input, 45), (Binary Input, 46), 

        (Binary Input, 47), (Binary Input, 48), (Binary Input, 49), (Binary Input, 50), 

        (Binary Input, 51), (Binary Input, 52), (Binary Input, 53), (Binary Input, 54), 

        (Binary Input, 55), (Binary Input, 56), (Binary Input, 57), (Binary Input, 58), 

        (Binary Input, 59), (Binary Input, 60), (Binary Input, 61), (Binary Input, 62), 

        (Binary Input, 63), (Binary Output, 0), (Binary Output, 1), (Binary Output, 2), 

        (Binary Output, 3), (Binary Output, 4), (Binary Output, 5), (Binary Output, 6), 

        (Binary Output, 7), (Binary Output, 8), (Binary Output, 9), (Binary Output, 10), 

        (Binary Output, 11), (Binary Output, 12), (Binary Output, 13), (Binary Output, 14), 

        (Binary Output, 15), (Binary Output, 16), (Binary Output, 17), (Binary Output, 18), 

        (Binary Output, 19), (Binary Output, 20), (Binary Output, 21), (Binary Output, 22), 

        (Binary Output, 23), (Binary Output, 24), (Binary Output, 25), (Binary Output, 26), 

        (Binary Output, 27), (Binary Output, 28), (Binary Output, 29), (Binary Output, 30), 

        (Binary Output, 31), (Binary Output, 32), (Binary Output, 33), (Binary Output, 34), 

        (Binary Output, 35), (Binary Output, 36), (Binary Output, 37), (Binary Output, 38), 

        (Binary Output, 39), (Binary Output, 40), (Binary Output, 41), (Binary Output, 42), 

        (Binary Output, 43), (Binary Output, 44), (Binary Output, 45), (Binary Output, 46), 

        (Binary Output, 47), (Binary Output, 48), (Binary Output, 49), (Binary Output, 50), 

        (Binary Output, 51), (Binary Output, 52), (Binary Output, 53), (Binary Output, 54), 

        (Binary Output, 55), (Binary Output, 56), (Binary Output, 57), (Binary Output, 58), 

        (Binary Output, 59), (Binary Output, 60), (Binary Output, 61), (Binary Output, 62), 

        (Binary Output, 63) } 

    max-apdu-length-accepted: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
1476

    segmentation-supported: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
no-segmentation

    apdu-timeout: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
3000

    number-of-APDU-retries: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
3

    device-address-binding: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
?

    database-revision: BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
3

  -- Found 257 Objects 

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 0)

    object-name: "Temp_Chiller1"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "Temp_Chiller1"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 1)

    object-name: "Temp_Tower1"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "Temp_Tower1"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 2)

    object-name: "Temp_Ambient1"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "Temp_Ambient1"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 3)

    object-name: "Temp_Floor1"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "Temp_Floor1"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 4)

    object-name: "Humidity_Ambient1"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "Humidity_Ambient1"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 5)

    object-name: "ANALOG INPUT 5"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 5"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 6)

    object-name: "ANALOG INPUT 6"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 6"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 7)

    object-name: "ANALOG INPUT 7"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 7"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 8)

    object-name: "ANALOG INPUT 8"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 8"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 9)

    object-name: "ANALOG INPUT 9"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 9"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 10)

    object-name: "ANALOG INPUT 10"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 10"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 11)

    object-name: "ANALOG INPUT 11"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 11"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 12)

    object-name: "ANALOG INPUT 12"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 12"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 13)

    object-name: "ANALOG INPUT 13"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 13"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 14)

    object-name: "ANALOG INPUT 14"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 14"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 15)

    object-name: "ANALOG INPUT 15"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 15"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 16)

    object-name: "ANALOG INPUT 16"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 16"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 17)

    object-name: "ANALOG INPUT 17"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 17"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 18)

    object-name: "ANALOG INPUT 18"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 18"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 19)

    object-name: "ANALOG INPUT 19"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 19"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 20)

    object-name: "ANALOG INPUT 20"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 20"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 21)

    object-name: "ANALOG INPUT 21"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 21"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 22)

    object-name: "ANALOG INPUT 22"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 22"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 23)

    object-name: "ANALOG INPUT 23"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 23"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 24)

    object-name: "ANALOG INPUT 24"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 24"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 25)

    object-name: "ANALOG INPUT 25"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 25"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 26)

    object-name: "ANALOG INPUT 26"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 26"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 27)

    object-name: "ANALOG INPUT 27"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 27"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 28)

    object-name: "ANALOG INPUT 28"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 28"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 29)

    object-name: "ANALOG INPUT 29"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 29"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 30)

    object-name: "ANALOG INPUT 30"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 30"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 31)

    object-name: "ANALOG INPUT 31"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 31"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 32)

    object-name: "ANALOG INPUT 32"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 32"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 33)

    object-name: "ANALOG INPUT 33"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 33"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 34)

    object-name: "ANALOG INPUT 34"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 34"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 35)

    object-name: "ANALOG INPUT 35"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 35"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 36)

    object-name: "ANALOG INPUT 36"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 36"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 37)

    object-name: "ANALOG INPUT 37"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 37"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 38)

    object-name: "ANALOG INPUT 38"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 38"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 39)

    object-name: "ANALOG INPUT 39"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 39"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 40)

    object-name: "ANALOG INPUT 40"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 40"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 41)

    object-name: "ANALOG INPUT 41"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 41"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 42)

    object-name: "ANALOG INPUT 42"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 42"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 43)

    object-name: "ANALOG INPUT 43"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 43"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 44)

    object-name: "ANALOG INPUT 44"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 44"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 45)

    object-name: "ANALOG INPUT 45"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 45"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 46)

    object-name: "ANALOG INPUT 46"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 46"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 47)

    object-name: "ANALOG INPUT 47"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 47"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 48)

    object-name: "ANALOG INPUT 48"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 48"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 49)

    object-name: "ANALOG INPUT 49"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 49"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 50)

    object-name: "ANALOG INPUT 50"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 50"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 51)

    object-name: "ANALOG INPUT 51"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 51"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 52)

    object-name: "ANALOG INPUT 52"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 52"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 53)

    object-name: "ANALOG INPUT 53"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 53"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 54)

    object-name: "ANALOG INPUT 54"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 54"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 55)

    object-name: "ANALOG INPUT 55"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 55"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 56)

    object-name: "ANALOG INPUT 56"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 56"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 57)

    object-name: "ANALOG INPUT 57"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 57"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 58)

    object-name: "ANALOG INPUT 58"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 58"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 59)

    object-name: "ANALOG INPUT 59"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 59"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 60)

    object-name: "ANALOG INPUT 60"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 60"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 61)

    object-name: "ANALOG INPUT 61"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 61"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 62)

    object-name: "ANALOG INPUT 62"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 62"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Input, 63)

    object-name: "ANALOG INPUT 63"

    object-type: Analog Input

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    description: "ANALOG INPUT 63"

    reliability: no-fault-detected

    proprietary 9997: 90.510002

    proprietary 9998: 90

    proprietary 9999: -200

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 0)

    object-name: "Temp_SP1"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "Temp_SP1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 1)

    object-name: "Fan_Speed1"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "Fan_Speed1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 2)

    object-name: "Pump_Speed1"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "Pump_Speed1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 3)

    object-name: "ANALOG OUTPUT 3"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 3"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 4)

    object-name: "ANALOG OUTPUT 4"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 4"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 5)

    object-name: "ANALOG OUTPUT 5"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 5"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 6)

    object-name: "ANALOG OUTPUT 6"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 6"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 7)

    object-name: "ANALOG OUTPUT 7"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 7"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 8)

    object-name: "ANALOG OUTPUT 8"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 8"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 9)

    object-name: "ANALOG OUTPUT 9"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 9"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 10)

    object-name: "ANALOG OUTPUT 10"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 10"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 11)

    object-name: "ANALOG OUTPUT 11"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 11"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 12)

    object-name: "ANALOG OUTPUT 12"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 12"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 13)

    object-name: "ANALOG OUTPUT 13"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 13"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 14)

    object-name: "ANALOG OUTPUT 14"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 14"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 15)

    object-name: "ANALOG OUTPUT 15"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 15"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 16)

    object-name: "ANALOG OUTPUT 16"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 16"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 17)

    object-name: "ANALOG OUTPUT 17"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 17"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 18)

    object-name: "ANALOG OUTPUT 18"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 18"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 19)

    object-name: "ANALOG OUTPUT 19"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 19"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 20)

    object-name: "ANALOG OUTPUT 20"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 20"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 21)

    object-name: "ANALOG OUTPUT 21"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 21"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 22)

    object-name: "ANALOG OUTPUT 22"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 22"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 23)

    object-name: "ANALOG OUTPUT 23"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 23"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 24)

    object-name: "ANALOG OUTPUT 24"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 24"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 25)

    object-name: "ANALOG OUTPUT 25"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 25"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 26)

    object-name: "ANALOG OUTPUT 26"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 26"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 27)

    object-name: "ANALOG OUTPUT 27"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 27"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 28)

    object-name: "ANALOG OUTPUT 28"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 28"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 29)

    object-name: "ANALOG OUTPUT 29"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 29"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 30)

    object-name: "ANALOG OUTPUT 30"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 30"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 31)

    object-name: "ANALOG OUTPUT 31"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 31"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 32)

    object-name: "ANALOG OUTPUT 32"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 32"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 33)

    object-name: "ANALOG OUTPUT 33"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 33"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 34)

    object-name: "ANALOG OUTPUT 34"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 34"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 35)

    object-name: "ANALOG OUTPUT 35"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 35"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 36)

    object-name: "ANALOG OUTPUT 36"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 36"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 37)

    object-name: "ANALOG OUTPUT 37"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 37"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 38)

    object-name: "ANALOG OUTPUT 38"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 38"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 39)

    object-name: "ANALOG OUTPUT 39"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 39"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 40)

    object-name: "ANALOG OUTPUT 40"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 40"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 41)

    object-name: "ANALOG OUTPUT 41"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 41"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 42)

    object-name: "ANALOG OUTPUT 42"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 42"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 43)

    object-name: "ANALOG OUTPUT 43"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 43"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 44)

    object-name: "ANALOG OUTPUT 44"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 44"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 45)

    object-name: "ANALOG OUTPUT 45"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 45"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 46)

    object-name: "ANALOG OUTPUT 46"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 46"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 47)

    object-name: "ANALOG OUTPUT 47"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 47"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 48)

    object-name: "ANALOG OUTPUT 48"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 48"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 49)

    object-name: "ANALOG OUTPUT 49"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 49"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 50)

    object-name: "ANALOG OUTPUT 50"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 50"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 51)

    object-name: "ANALOG OUTPUT 51"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 51"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 52)

    object-name: "ANALOG OUTPUT 52"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 52"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 53)

    object-name: "ANALOG OUTPUT 53"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 53"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 54)

    object-name: "ANALOG OUTPUT 54"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 54"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 55)

    object-name: "ANALOG OUTPUT 55"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 55"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 56)

    object-name: "ANALOG OUTPUT 56"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 56"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 57)

    object-name: "ANALOG OUTPUT 57"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 57"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 58)

    object-name: "ANALOG OUTPUT 58"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 58"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 59)

    object-name: "ANALOG OUTPUT 59"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 59"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 60)

    object-name: "ANALOG OUTPUT 60"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 60"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 61)

    object-name: "ANALOG OUTPUT 61"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 61"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 62)

    object-name: "ANALOG OUTPUT 62"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 62"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Analog Output, 63)

    object-name: "ANALOG OUTPUT 63"

    object-type: Analog Output

    present-value: 0.000000

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    units: no-units

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: 0.000000

    description: "ANALOG OUTPUT 63"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 0)

    object-name: "Tower_FLT1"

    object-type: Binary Input

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "Tower_FLT1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 1)

    object-name: "Chiller_FLT1"

    object-type: Binary Input

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "Chiller_FLT1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 2)

    object-name: "Occupied_1"

    object-type: Binary Input

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "Occupied_1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 3)

    object-name: "Tower_AUTO1"

    object-type: Binary Input

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "Tower_AUTO1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 4)

    object-name: "Tower_HAND1"

    object-type: Binary Input

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "Tower_HAND1"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 5)

    object-name: "IntoBackWash"

    object-type: Binary Input

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "IntoBackWash"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 6)

    object-name: "BINARY INPUT 6"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 6"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 7)

    object-name: "BINARY INPUT 7"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 7"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 8)

    object-name: "BINARY INPUT 8"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 8"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 9)

    object-name: "BINARY INPUT 9"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 9"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 10)

    object-name: "BINARY INPUT 10"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 10"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 11)

    object-name: "BINARY INPUT 11"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 11"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 12)

    object-name: "BINARY INPUT 12"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 12"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 13)

    object-name: "BINARY INPUT 13"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 13"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 14)

    object-name: "BINARY INPUT 14"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 14"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 15)

    object-name: "BINARY INPUT 15"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 15"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 16)

    object-name: "BINARY INPUT 16"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 16"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 17)

    object-name: "BINARY INPUT 17"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 17"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 18)

    object-name: "BINARY INPUT 18"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 18"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 19)

    object-name: "BINARY INPUT 19"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 19"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 20)

    object-name: "BINARY INPUT 20"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 20"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 21)

    object-name: "BINARY INPUT 21"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 21"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 22)

    object-name: "BINARY INPUT 22"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 22"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 23)

    object-name: "BINARY INPUT 23"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 23"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 24)

    object-name: "BINARY INPUT 24"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 24"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 25)

    object-name: "BINARY INPUT 25"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 25"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 26)

    object-name: "BINARY INPUT 26"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 26"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 27)

    object-name: "BINARY INPUT 27"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 27"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 28)

    object-name: "BINARY INPUT 28"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 28"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 29)

    object-name: "BINARY INPUT 29"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 29"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 30)

    object-name: "BINARY INPUT 30"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 30"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 31)

    object-name: "BINARY INPUT 31"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 31"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 32)

    object-name: "BINARY INPUT 32"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 32"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 33)

    object-name: "BINARY INPUT 33"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 33"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 34)

    object-name: "BINARY INPUT 34"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 34"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 35)

    object-name: "BINARY INPUT 35"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 35"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 36)

    object-name: "BINARY INPUT 36"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 36"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 37)

    object-name: "BINARY INPUT 37"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 37"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 38)

    object-name: "BINARY INPUT 38"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 38"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 39)

    object-name: "BINARY INPUT 39"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 39"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 40)

    object-name: "BINARY INPUT 40"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 40"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 41)

    object-name: "BINARY INPUT 41"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 41"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 42)

    object-name: "BINARY INPUT 42"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 42"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 43)

    object-name: "BINARY INPUT 43"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 43"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 44)

    object-name: "BINARY INPUT 44"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 44"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 45)

    object-name: "BINARY INPUT 45"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 45"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 46)

    object-name: "BINARY INPUT 46"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 46"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 47)

    object-name: "BINARY INPUT 47"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 47"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 48)

    object-name: "BINARY INPUT 48"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 48"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 49)

    object-name: "BINARY INPUT 49"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 49"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 50)

    object-name: "BINARY INPUT 50"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 50"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 51)

    object-name: "BINARY INPUT 51"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 51"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 52)

    object-name: "BINARY INPUT 52"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 52"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 53)

    object-name: "BINARY INPUT 53"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 53"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 54)

    object-name: "BINARY INPUT 54"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 54"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 55)

    object-name: "BINARY INPUT 55"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 55"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 56)

    object-name: "BINARY INPUT 56"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 56"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 57)

    object-name: "BINARY INPUT 57"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 57"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 58)

    object-name: "BINARY INPUT 58"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 58"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 59)

    object-name: "BINARY INPUT 59"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 59"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 60)

    object-name: "BINARY INPUT 60"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 60"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 61)

    object-name: "BINARY INPUT 61"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 61"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 62)

    object-name: "BINARY INPUT 62"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 62"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Input, 63)

    object-name: "BINARY INPUT 63"

    object-type: Binary Input

    present-value: active

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    description: "BINARY INPUT 63"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 0)

    object-name: "Floor_Enable1"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "Floor_Enable1"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 1)

    object-name: "Floor_Heat1"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "Floor_Heat1"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 2)

    object-name: "Floor_Cool1"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "Floor_Cool1"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 3)

    object-name: "BINARY OUTPUT 3"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 3"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 4)

    object-name: "BINARY OUTPUT 4"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 4"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 5)

    object-name: "BINARY OUTPUT 5"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 5"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 6)

    object-name: "BINARY OUTPUT 6"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 6"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 7)

    object-name: "BINARY OUTPUT 7"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 7"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 8)

    object-name: "BINARY OUTPUT 8"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 8"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 9)

    object-name: "BINARY OUTPUT 9"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 9"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 10)

    object-name: "BINARY OUTPUT 10"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 10"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 11)

    object-name: "BINARY OUTPUT 11"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 11"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 12)

    object-name: "BINARY OUTPUT 12"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 12"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 13)

    object-name: "BINARY OUTPUT 13"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 13"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 14)

    object-name: "BINARY OUTPUT 14"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 14"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 15)

    object-name: "BINARY OUTPUT 15"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 15"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 16)

    object-name: "BINARY OUTPUT 16"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 16"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 17)

    object-name: "BINARY OUTPUT 17"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 17"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 18)

    object-name: "BINARY OUTPUT 18"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 18"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 19)

    object-name: "BINARY OUTPUT 19"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 19"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 20)

    object-name: "BINARY OUTPUT 20"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 20"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 21)

    object-name: "BINARY OUTPUT 21"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 21"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 22)

    object-name: "BINARY OUTPUT 22"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 22"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 23)

    object-name: "BINARY OUTPUT 23"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 23"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 24)

    object-name: "BINARY OUTPUT 24"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 24"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 25)

    object-name: "BINARY OUTPUT 25"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 25"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 26)

    object-name: "BINARY OUTPUT 26"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 26"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 27)

    object-name: "BINARY OUTPUT 27"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 27"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 28)

    object-name: "BINARY OUTPUT 28"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 28"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 29)

    object-name: "BINARY OUTPUT 29"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 29"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 30)

    object-name: "BINARY OUTPUT 30"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 30"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 31)

    object-name: "BINARY OUTPUT 31"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 31"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 32)

    object-name: "BINARY OUTPUT 32"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 32"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 33)

    object-name: "BINARY OUTPUT 33"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 33"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 34)

    object-name: "BINARY OUTPUT 34"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 34"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 35)

    object-name: "BINARY OUTPUT 35"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 35"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 36)

    object-name: "BINARY OUTPUT 36"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 36"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 37)

    object-name: "BINARY OUTPUT 37"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 37"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 38)

    object-name: "BINARY OUTPUT 38"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 38"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 39)

    object-name: "BINARY OUTPUT 39"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 39"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 40)

    object-name: "BINARY OUTPUT 40"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 40"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 41)

    object-name: "BINARY OUTPUT 41"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 41"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 42)

    object-name: "BINARY OUTPUT 42"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 42"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 43)

    object-name: "BINARY OUTPUT 43"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 43"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 44)

    object-name: "BINARY OUTPUT 44"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 44"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 45)

    object-name: "BINARY OUTPUT 45"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 45"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 46)

    object-name: "BINARY OUTPUT 46"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 46"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 47)

    object-name: "BINARY OUTPUT 47"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 47"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 48)

    object-name: "BINARY OUTPUT 48"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 48"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 49)

    object-name: "BINARY OUTPUT 49"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 49"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 50)

    object-name: "BINARY OUTPUT 50"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 50"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 51)

    object-name: "BINARY OUTPUT 51"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 51"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 52)

    object-name: "BINARY OUTPUT 52"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 52"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 53)

    object-name: "BINARY OUTPUT 53"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 53"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 54)

    object-name: "BINARY OUTPUT 54"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 54"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 55)

    object-name: "BINARY OUTPUT 55"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 55"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 56)

    object-name: "BINARY OUTPUT 56"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 56"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 57)

    object-name: "BINARY OUTPUT 57"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 57"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 58)

    object-name: "BINARY OUTPUT 58"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 58"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 59)

    object-name: "BINARY OUTPUT 59"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 59"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 60)

    object-name: "BINARY OUTPUT 60"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 60"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 61)

    object-name: "BINARY OUTPUT 61"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 61"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 62)

    object-name: "BINARY OUTPUT 62"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 62"

    active-text: "on"

    inactive-text: "off"

  }, 

  { 

BVLC: Sent Original-Unicast-NPDU.
BVLC: Received Original-Unicast-NPDU.
    object-identifier: (Binary Output, 63)

    object-name: "BINARY OUTPUT 63"

    object-type: Binary Output

    present-value: inactive

    status-flags: {false,false,false,false}

    event-state: normal

    out-of-service: FALSE

    polarity: normal

    priority-array: { Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null,Null }

    relinquish-default: inactive

    description: "BINARY OUTPUT 63"

    active-text: "on"

    inactive-text: "off"

  } 

} 

End of BACnet Protocol Implementation Conformance Statement