Usage: bacrd device-instance state [password]
Send BACnet ReinitializeDevice service to device.

The device-instance can be 0 to 4194302.
Possible state values:
  0=coldstart
  1=warmstart
  2=startbackup
  3=endbackup
  4=startrestore
  5=endrestore
  6=abortrestore
The optional password is a character string of 1 to 20 characters.